P a g a n i    Z  O  N  D  A    C 1 2 S
________________________________________
Original model for NFS4 by FiVESPEED


Converting to NFS6 by 'R - R' :

RobinCZ - ALL(except one important thing)
ROM - windows (<= the important thing;o))

webpage : http://r-r.webz.cz

----------------------------------------

Pagani Zonda C12S specifications:

Engine Mercedes–Benz M 120 E 72 AMG
12 cylinder V 60° displacement 7010 cc 
Power: 550 BHP at 5550 RPM
Torque: 750 NM at 4100 RPM

Brakes Brembo
Front: Ventilated disk Ć 355 (14 in.)
Four piston caliper
Rear: Ventilated disk Ć 335 (14 in.)
Four piston caliper
Hydraulic power brakes

Transmission
Engine longitudinal center-rear
Rear wheel drive
AP twin plate clutch
Mechanical 6 speed (+reverse) gearbox
Self locking differential

Suspension
Independent wheels with double A-arm
Helical spring and hydraulic dampers – anti-roll bar
Suspension arms in aluminum alloy

Wheels
Aluminum alloy OZ wheels
Michelin Pilot tires
Front: 255/40/18
Rear: 345/35/18

Structure
Central carbon fiber chassis. 
Front and rear frame: Cr Mo steel space frame 
Carbon fiber -MD system- body panels

Performance
Top Speed : over 330 KPH
0 - 100 KPH : ~ 3.5 seconds
0 - 160 KPH : N/A

Price : 350,000 USD





